/ ****
MODEL: ZH-A1
A maximum number of points: 20480 (color area halved)
     Monochrome: 16 * 128 032 * 640
           48 * 424
     Color: 16 * 64 032 * 320
           48 * 208
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports serial communications mode
8. Supports serial program upgrade
9 RS-232 communication lines as straight lines
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5

/ ****
MODEL: ZH-A4
A maximum number of points: 65536 (color area halved)
     Monochrome: 16 * 409 632 * 2048
           48 * 136 064 * 1024
     Color: 16 * 204 832 * 1024
           48 * 68 064 * 512
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports serial communications mode
8. Supports serial program upgrade
9 RS-232 communication lines as straight lines
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-U0
A maximum number of points: 25600 (color area halved)
     Monochrome: 16 * 160 032 * 800
     Color: 16 * 80 032 * 400
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5

/ ****
MODEL: ZH-Um
A maximum number of points: 16384 (color area halved)
     Monochrome: 16 * 102 432 * 512
     Color: 16 * 51 232 * 256
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-U1
A maximum number of points: 32768 (color area halved)
     Monochrome: 16 * 204 832 * 1024
           48 * 680
     Color: 16 * 102 432 * 512
           48 * 336
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-U2
A maximum number of points: 49152 (color area halved)
     Monochrome: 16 * 307 232 * 1536
           48 * 102 464 * 768
     Color: 16 * 153 632 * 768
           48 * 51 264 * 384
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-U3
A maximum number of points: 65536 (color area halved)
     Monochrome: 16 * 409 632 * 2048
           48 * 136 064 * 1024
           80 * 81 696 * 680
           128 * 512
     Color: 16 * 204 832 * 1024
           48 * 68 064 * 512
           80 * 40 896 * 336
           128 * 256
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
          PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-U4
1 Maximum Points: 102400 (color area halved)
     Monochrome: 16 * 409 632 * 3200
           48 * 212 864 * 1600
           80 * 128 096 * 1064
           128 * 800
     Color: 16 * 320 032 * 1600
           48 * 106 464 * 800
           80 * 64 096 * 528
           128 * 400
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-UF
A maximum number of points: 24576 (color area halved)
     Monochrome: 16 * 153 632 * 768
           48 * 51 264 * 384
     Color: 16 * 76 832 * 384
           48 * 25 664 * 192
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-U5
1 Maximum Points: 163840 (color half-height)
     Monochrome: 16 * 409 632 * 409 648 * 300 864 * 2560
           80 * 204896 * 1704128 * 1280144 * 1136
           160 * 1024 176 * 928 192 * 848 208 * 784
           224 * 728 240 * 680 256 * 640
     Color: 16 * 409 632 * 204 848 * 169 664 * 1280
           80 * 102 496 * 848 128 * 640
   Note: 12 Interface with 8 rows high 08 interfaces with 4 rows high

2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
Model: ZH-U6
1 Maximum Points: 524288 (color area halved)
     Monochrome: 32 * 409 664 * 409 696 * 4096 128 * 4096
           144 * 3640160 * 3272176 * 2976192 * 2728
           208 * 2520224 * 2336240 * 2184256 * 2048
     Color: 32 * 409 664 * 409 696 * 2728128 * 2048
           144 * 1816160 * 1632176 * 1488192 * 1360
           208 * 1256224 * 1168240 * 1088256 * 1024
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5


/ ****
Model: ZH-U8
A maximum number of points: 1048576 (color area halved)
     Monochrome: 32 * 819 264 * 819 296 * 8192128 * 8192
           160 * 6552192 * 5456208 * 5040224 * 4680
           240 * 4368256 * 4096288 * 3640320 * 3272
           352 * 2976384 * 2728416 * 2520448 * 2336
           480 * 2184512 * 2048
     Color: 32 * 819 264 * 819 296 * 5456128 * 4096
           160 * 3272192 * 2728224 * 2336256 * 2048
           288 * 1816320 * 1632352 * 1488384 * 1360
           416 * 1256448 * 1168480 * 1088512 * 1024
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-E1
A maximum number of points: 32768 (color area halved)
     Monochrome: 16 * 204 832 * 1024
           48 * 680
     Color: 16 * 102 432 * 512
           48 * 336
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports dual Ethernet port and serial communication mode
8. Automatically obtain IP, IP settings without
9. Supports stand-alone and LAN communications directly connected
10. Communication network port fully compatible straight lines and cross lines
11 RS-232 serial communication for the straight line
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5


/ ****
MODEL: ZH-E3
A maximum number of points: 65536 (color area halved)
     Monochrome: 16 * 409 632 * 2048
           48 * 136 064 * 1024
           80 * 81 696 * 680
           128 * 512
     Color: 16 * 204 832 * 1024
           48 * 68 064 * 512
           80 * 40 896 * 336
           128 * 256
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports dual Ethernet port and serial communication mode
8. Automatically obtain IP, IP settings without
9. Supports stand-alone and LAN communications directly connected
10. Communication network port fully compatible straight lines and cross lines
11 RS-232 serial communication for the straight line
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-E5
1 Maximum Points: 163840 (color half-height)
     Monochrome: 16 * 409 632 * 409 648 * 300 864 * 2560
           80 * 204896 * 1704128 * 1280144 * 1136
           160 * 1024 176 * 928 192 * 848 208 * 784
           224 * 728 240 * 680 256 * 640
     Color: 16 * 409 632 * 204 848 * 169 664 * 1280
           80 * 102 496 * 848 128 * 640
   Note: 12 Interface with 8 rows high 08 interfaces with 4 rows high
     
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports dual Ethernet port and serial communication mode
8. Automatically obtain IP, IP settings without
9. Supports stand-alone and LAN communications directly connected
10. Communication network port fully compatible straight lines and cross lines
11 RS-232 serial communication for the straight line
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-E6

1 Maximum Points: 524288 (color area halved)
     Monochrome: 32 * 409 664 * 409 696 * 4096 128 * 4096
           144 * 3640160 * 3272176 * 2976192 * 2728
           208 * 2520224 * 2336240 * 2184256 * 2048
     Color: 32 * 409 664 * 409 696 * 2728128 * 2048
           144 * 1816160 * 1632176 * 1488192 * 1360
           208 * 1256224 * 1168240 * 1088256 * 1024
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports dual Ethernet port and serial communication mode
8. Automatically obtain IP, IP settings without
9. Supports stand-alone and LAN communications directly connected
10. Communication network port fully compatible straight lines and cross lines
11 RS-232 serial communication for the straight line
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-E8
A maximum number of points: 1048576 (color area halved)
     Monochrome: 32 * 819 264 * 819 296 * 8192128 * 8192
           160 * 6552192 * 5456208 * 5040224 * 4680
           240 * 4368256 * 4096288 * 3640320 * 3272
           352 * 2976384 * 2728416 * 2520448 * 2336
           480 * 2184512 * 2048
     Color: 32 * 819 264 * 819 296 * 5456128 * 4096
           160 * 3272192 * 2728224 * 2336256 * 2048
           288 * 1816320 * 1632352 * 1488384 * 1360
           416 * 1256448 * 1168480 * 1088512 * 1024
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports dual Ethernet port and serial communication mode
8. Automatically obtain IP, IP settings without
9. Supports stand-alone and LAN communications directly connected
10. Communication network port fully compatible straight lines and cross lines
11 RS-232 serial communication for the straight line
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-Gm
A maximum number of points: 16384 (color area halved)
     Monochrome: 16 * 1024
     Color: 16 * 512
(2) support 1/4, 1/8, 1/16
3 support free partition
4 Support magical run side (the entire screen / partition)
5 Support countdown, temperature
6 communication interfaces:. GPRS RS-232
7. Timer switch support
8. Full screen test support
9 RS-232 communication lines as straight lines
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-G0
A maximum number of points: 25600 (color area halved)
     Monochrome: 16 * 160 032 * 800
     Color: 16 * 80 032 * 400
(2) support 1/4, 1/8, 1/16
3 support free partition
4 Support magical run side (the entire screen / partition)
5 Support countdown, temperature
6 communication interfaces:. GPRS RS-232
7. Timer switch support
8. Full screen test support
9 RS-232 communication lines as straight lines
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5
/ ****
MODEL: ZH-G3
A maximum number of points: 65536 (color area halved)
     Monochrome: 16 * 409 632 * 2048
           48 * 136 064 * 1024
           80 * 81 696 * 680
           128 * 512
     Color: 16 * 204 832 * 1024
           48 * 68 064 * 512
           80 * 40 896 * 336
           128 * 256
(2) support 1/4, 1/8, 1/16
3 support free partition
4 Support magical run side (the entire screen / partition)
5 Support countdown, temperature
6 communication interfaces:. GPRS RS-232
7. Timer switch support
8. Full screen test support
9 RS-232 communication lines as straight lines
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5


/ ****
Model: ZH-U7
1 Maximum Points: 524288 (color area halved)
     Monochrome: 32 * 409 664 * 409 696 * 4096 128 * 4096
           160 * 3272192 * 2728224 * 2336256 * 2048
           288 * 1816320 * 1632352 * 1488384 * 1360
           416 * 1256448 * 1168480 * 1088512 * 1024
     Color: 32 * 409 664 * 409 696 * 2728128 * 2048
           160 * 1632192 * 1360224 * 1168256 * 1024
           288 * 904 320 * 816 352 * 744 384 * 680
           416 * 624 448 * 584 480 * 544 512 * 512
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7 Support U disk and dual serial communication mode
8 and serial port support U disk upgrade
9. Supports all U disk storage format FAT32/NTFS/EXFAT
10. Communication line RS-232 straight cable
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5

/ ****
MODEL: ZH-E7

1 Maximum Points: 524288 (color area halved)
     Monochrome: 32 * 409 664 * 409 696 * 4096 128 * 4096
           160 * 3272192 * 2728224 * 2336256 * 2048
           288 * 1816320 * 1632352 * 1488384 * 1360
           416 * 1256448 * 1168480 * 1088512 * 1024
     Color: 32 * 409 664 * 409 696 * 2728128 * 2048
           160 * 1632192 * 1360224 * 1168256 * 1024
           288 * 904 320 * 816 352 * 744 384 * 680
           416 * 624 448 * 584 480 * 544 512 * 512
2 supports all scanning
3 supports 16 free partition
4 supports the entire screen and run side by side partitions running
5 support full screen dynamic background and dynamic context by district
6 N kinds of cool text animation support
7. Supports dual Ethernet port and serial communication mode
8. Automatically obtain IP, IP settings without
9. Supports stand-alone and LAN communications directly connected
10. Communication network port fully compatible straight lines and cross lines
11 RS-232 serial communication for the straight line
   Connection as follows
         PC ---- Device
          2 ---- 2
          3 ---- 3
          5 ---- 5