{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":185,"n_cols":7,"rows_kept":185,"cut":false,"hidden":false,"merged":[[1,2,1,5],[4,2,4,5],[6,2,6,3],[2,2,2,6],[3,2,3,5]]}
[null,null,"ООО \"Евразия Снаб\""]
[null,null,"660118, г. Красноярск, Северное шоссе, 17К, оф. 308"]
[null,null,"ИНН 2464230865 / КПП 246601001 / ОГРН 1102468060265"]
[null,null,"тел. (391) 214-69-88, 215-22-69"]
[null,null,"E-mail: smk24@list.ru      Сайт: eurasia-snab.ru"]
[]
[null,null,"Прайс-лист от 27.04.2017 г."]
[]
["Наименование","Марка стали","Размер (м)","Цена за тонну","Цена за штуку","Вес штуки","Вес метра"]
["Арматура AIII, ГОСТ 5781-82"]
["Ø 10","35ГС",11.7,35000.0,{"$f":"(D11+D11*5%)/(1000/F11)","v":290.325},{"$f":"ROUNDUP(G11*C11,1)","v":7.9},0.67]
["Ø 12","35ГС",11.7,35000.0,400.575,10.9,0.93]
["Ø 14 ","35ГС",11.7,35000.0,562.275,15.3,1.3]
["Ø 16 ","35ГС",11.7,35000.0,716.625,19.5,1.66]
["Ø 18","35ГС",11.7,35000.0,904.05,24.6,2.1]
["Ø 20","35ГС",11.7,35000.0,1076.775,29.3,2.5]
["Ø 8","25Г2С",6.0,41500.0,122.01,2.8,0.46]
["Ø 10","25Г2С, А500С",11.7,36000.0,306.18,8.1,0.69]
["Ø 12","25Г2С, А500С",11.7,36000.0,412.02,10.9,0.93]
["Ø 14","25Г2С, А500С",11.7,36000.0,578.34,15.3,1.3]
["Ø 16","25Г2С, А500С",11.7,36000.0,737.1,19.5,1.66]
["Ø 18","25Г2С, А500С",11.7,36000.0,{"$f":"(D22+D22*3%)/(1000/F22)","v":912.168},24.6,2.1]
["Ø 20","25Г2С, А500С",11.7,36000.0,1086.444,29.3,2.5]
["Ø 25","25Г2С, А500С",11.7,37000.0,1783.548,46.8,4.0]
["Балка двутавровая, ГОСТ 26020-83, ГОСТ 8239, СТО-АСЧМ"]
[10.0,"Ст.3пс",12.0,52000.0,{"$f":"(D26+D26*3%)/(1000/F26)","v":6491.472},{"$f":"ROUNDUP(G26*C26,1)","v":121.2},10.1]
["12Б1","Ст.3пс",11.7,54000.0,8009.28,144,12.3]
[14.0,"Ст.3пс",12.0,50000.0,8837.4,171.6,14.3]
["14Б1","Ст.3пс",11.7,53000.0,7282.306,133.4,11.4]
["16Б1","Ст.3пс",11.7,50000.0,7956.75,154.5,13.2]
["18Б1","Ст.3пс",12.0,50000.0,9949.8,193.2,16.1]
["20Б1","Ст.3пс",12.0,64000.0,18431.232,279.6,23.3]
["20К1","Ст.3пс",12.0,64000.0,33302.784,505.2,42.1]
["20Ш1","Ст.3пс",12.0,67000.0,26002.968,376.8,31.4]
["25Б1","Ст.3пс",12.0,67000.0,21779.556,315.6,26.3]
["25К1","Ст.3пс",12.0,65000.0,50774.88,758.4,63.2]
["25Ш1","Ст.3пс",12.0,67000.0,37016.964,536.4,44.7]
["30Б1","Ст.3пс",12.0,66000.0,26022.744,382.8,31.9]
["30К1","Ст.3пс",12.0,65000.0,70377.84,1051.2,87.6]
["30Ш1","Ст.3пс",12.0,67000.0,47616.9,690,57.5]
["35Б1","Ст.3пс",12.0,67000.0,32793.552,475.2,39.6]
["35К1","Ст.3пс",12.0,65000.0,88132.98,1316.4,109.7]
["35Ш1","Ст.3пс",12.0,67000.0,54821.544,794.4,66.2]
["40Б1","Ст.3пс",12.0,52000.0,31364.736,585.6,48.8]
["40Ш1","Ст.3пс",12.0,52000.0,57459.168,1072.8,89.4]
["45Б1","Ст.3пс",12.0,52000.0,38884.56,726,60.5]
["45Ш1","Ст.3пс",12.0,52000.0,79890.096,1491.6,124.3]
["45М","Ст.3пс",12.0,67000.0,65835.54,954,79.5]
["50Б1","Ст.3пс",12.0,52000.0,47432.736,885.6,73.8]
["Лист х/к, ГОСТ 16523-97, ГОСТ 19904-90"]
[0.5,"Ст.08пс","1.25х2.5",55000.0,{"$f":"(D51+D51*3%)/(1000/F51)","v":736.45},{"$f":"ROUNDUP(G51*(1.25*2.5),1)","v":13},4.15]
[0.7,"Ст.08пс","1.25х2.5",54000.0,1012.284,18.2,5.8]
[1.0,"Ст.08пс","1.25х2.5",53000.0,1386.586,25.4,8.1]
[1.2,"Ст.08пс","1.25х2.5",53000.0,1659.536,30.4,9.7]
[1.5,"Ст.08пс","1.25х2.5",53000.0,2030.748,37.2,11.9]
[2.0,"Ст.08пс","1.25х2.5",53000.0,2696.746,49.4,15.8]
[2.5,"Ст.08пс","1.25х2.5",53000.0,3433.711,62.9,20.1]
[3.0,"Ст.08пс","1.25х2.5",53000.0,4061.496,74.4,23.8]
["Лист г/к, ГОСТ 14637-89, ГОСТ 16523-97, ГОСТ 19903-74, ГОСТ 19281-89 (ст.09Г2С + 3000 руб/тн)"]
[2.0,"Ст.3сп5","1.25х2.5",46000.0,{"$f":"(D60+D60*3%)/(1000/F60)","v":2487.45},{"$f":"ROUNDUP(G60*(1.25*2.5),1)","v":52.5},16.8]
[2.5,"Ст.3сп5","1.25х2.5",46000.0,3065.486,64.7,20.7]
[3.0,"Ст.3сп5","1.25х2.5",46000.0,3733.544,78.8,25.2]
[4.0,"Ст.3сп5","1.5х6.0",45000.0,13807.665,{"$f":"ROUNDUP(G63*(1.5*6),1)","v":297.9},33.1]
[5.0,"Ст.3сп5","1.5х6.0",45000.0,16602.57,358.2,39.8]
[6.0,"Ст.3сп5","1.5х6.0",45000.0,19856.34,428.4,47.6]
[8.0,"Ст.3сп5","1.5х6.0",45000.0,26280.45,567,63.0]
[10.0,"Ст.3сп5","1.5х6.0",45000.0,32996.565,711.9,79.1]
[12.0,"Ст.3сп5","1.5х6.0",44500.0,38941.416,849.6,94.4]
[14.0,"Ст.3сп5","1.5х6.0",44500.0,45624.159,995.4,110.6]
[16.0,"Ст.3сп5","1.5х6.0",44500.0,52760.6685,1151.1,127.9]
[20.0,"Ст.3сп5","1.5х6.0",44500.0,65507.382,1429.2,158.8]
[25.0,"Ст.3сп5","1.5х6.0",44500.0,81966.7305,1788.3,198.7]
[30.0,"Ст.3сп5","1.5х6.0",44500.0,97353.54,2124,236.0]
[32.0,"Ст.3сп5","2.0х6.0",44500.0,140805.12,{"$f":"ROUNDUP(G74*(2*6),1)","v":3072},256.0]
[36.0,"Ст.3сп5","2.0х6.0",44500.0,159505.8,3480,290.0]
[40.0,"Ст.3сп5","1.5х6.0",44500.0,141492.645,{"$f":"ROUNDUP(G76*(1.5*6),1)","v":3087},343.0]
["Лист г/к, рифленый, ГОСТ 8568-77, ГОСТ 380-2005"]
["4,0 (чечевица)","Ст.3сп","1.5х6.0",48000.0,{"$f":"(D78+D78*3%)/(1000/F78)","v":14594.688},{"$f":"ROUNDUP(G78*(1.5*6),1)","v":295.2},32.8]
["5,0 (чечевица)","Ст.3сп","1.5х6.0",48000.0,18243.36,369,41.0]
["6,0 (чечевица)","Ст.3сп","1.5х6.0",48000.0,21847.536,441.9,49.1]
["Лист г/к, ПВЛ"]
[406.0,"Ст.3сп","1х2.2",50000.0,{"$f":"(D82+D82*3%)/(1000/F82)","v":2132.1},{"$f":"ROUNDUP(G82*(1*2.2),1)","v":41.4},18.8]
[408.0,"Ст.3сп","1х2.2",50000.0,2348.4,45.6,20.7]
[508.0,"Ст.3сп","1х2.2",50000.0,2755.25,53.5,24.3]
["Лист оцинкованный, ГОСТ 14918-80"]
[0.45,"Ст.08пс","1.25х2.5",64000.0,{"$f":"(D86+D86*3%)/(1000/F86)","v":764.672},{"$f":"ROUNDUP(G86*(1.25*2.5),1)","v":11.6},3.7]
[0.5,"Ст.08пс","1.25х2.5",57000.0,774.972,13.2,4.2]
[0.55,"Ст.08пс","1.25х2.5",57000.0,863.037,14.7,4.7]
[0.7,"Ст.08пс","1.25х2.5",57000.0,1068.522,18.2,5.8]
[0.8,"Ст.08пс","1.25х2.5",55000.0,1172.655,20.7,6.6]
[1.0,"Ст.08пс","1.25х2.5",54000.0,1412.748,25.4,8.1]
[1.5,"Ст.08пс","1.25х2.5",53000.0,2101.715,38.5,12.3]
[2.0,"Ст.08пс","1.25х2.5",57000.0,2976.597,50.7,16.2]
["Труба водогазопроводная, ГОСТ 3262-75"]
["Ø 15х2,8","Ст.3пс",6.0,50500.0,{"$f":"(D95+D95*3%)/(1000/F95)","v":436.926},{"$f":"ROUNDUP(G95*C95,1)","v":8.4},1.4]
["Ø 20х2,8","Ст.3пс",9.0,49500.0,871.8435,17.1,1.9]
["Ø 25х3,2","Ст.3пс",9.0,46000.0,1047.098,22.1,2.45]
["Ø 32х3,2","Ст.3пс",9.0,45000.0,1316.34,28.4,3.15]
["Ø 40х3,5","Ст.3пс",9.0,45000.0,1710.315,36.9,4.1]
["Ø 50х3,5","Ст.3пс",6.0,45000.0,1446.12,31.2,5.2]
["Труба электросварная, ГОСТ 10704-91"]
["Ø 57х3,5","Ст.3пс",11.7,45000.0,{"$f":"(D102+D102*3%)/(1000/F102)","v":2660.49},{"$f":"ROUNDUP(G102*C102,1)","v":57.4},4.9]
["Ø 76х3,5","Ст.3пс",11.7,45000.0,3527.235,76.1,6.5]
["Ø 89х3,5","Ст.3пс",11.7,45000.0,4125.15,89,7.6]
["Ø 108х3,5","Ст.3пс",11.7,45000.0,5209.74,112.4,9.6]
["Ø 114х4,0","Ст.3пс",11.7,46000.0,6268.374,132.3,11.3]
["Ø 127х4,0","Ст.3пс",11.7,46000.0,6988.55,147.5,12.6]
["Ø 133х4,0","Ст.3пс",11.7,45000.0,6998.85,151,12.9]
["Ø 159х4,5","Ст.3пс",11.7,46000.0,9869.254,208.3,17.8]
["Труба профильная, ГОСТ 8639-82, 8645-68"]
["15х15х1,5","Ст.2пс",6.0,52000.0,{"$f":"(D111+D111*3%)/(1000/F111)","v":235.664},{"$f":"ROUNDUP(G111*C111,1)","v":4.4},0.73]
["20х20х1,5","Ст.2пс",6.0,51500.0,312.9655,5.9,0.98]
["20х20х2,0","Ст.2пс",6.0,49000.0,363.384,7.2,1.2]
["25х25х1,5","Ст.2пс",6.0,51000.0,404.481,7.7,1.28]
["25х25х2,0","Ст.2пс",6.0,51000.0,472.77,9,1.5]
["30х20х1,5","Ст.2пс",6.0,51000.0,393.975,7.5,1.25]
["30х30х1,5","Ст.2пс",6.0,51000.0,472.77,9,1.5]
["40х20х1,5","Ст.2пс",6.0,51000.0,467.517,8.9,1.47]
["40х25х1,5","Ст.2пс",6.0,50000.0,504.7,9.8,1.62]
["40х25х2,0","Ст.2пс",6.0,50000.0,659.2,12.8,2.12]
["40х40х1,5","Ст.3пс",6.0,50000.0,643.75,12.5,2.08]
["40х40х2,0","Ст.3пс",6.0,49000.0,772.191,15.3,2.55]
["50х25х1,5","Ст.3пс",6.0,49000.0,575.358,11.4,1.9]
["50х25х2,0","Ст.3пс",6.0,49000.0,721.721,14.3,2.37]
["50х50х2,0","Ст.3пс",6.0,48000.0,934.416,18.9,3.15]
["50х50х3,0","Ст.3пс",6.0,48000.0,1320.048,26.7,4.45]
["60х30х2,0","Ст.3пс",6.0,48000.0,845.424,17.1,2.85]
["60х40х2,0","Ст.3пс",6.0,48000.0,934.416,18.9,3.15]
["60х60х2,0","Ст.3пс",6.0,48000.0,1142.064,23.1,3.85]
["80х60х3,0","Ст.3пс",12.0,46000.0,3809.352,80.4,6.7]
["80х80х3,0","Ст.3пс",12.0,45000.0,4143.69,89.4,7.45]
["80х80х4,0","Ст.3пс",12.0,45000.0,5339.52,115.2,9.6]
["100х100х3,0","Ст.3пс",12.0,45000.0,5228.28,112.8,9.4]
["100х100х4,0","Ст.3пс",12.0,45000.0,6785.64,146.4,12.2]
["120х120х4,0","Ст.3пс",12.0,46000.0,8357.832,176.4,14.7]
["140х140х5,0","Ст.3пс",12.0,50000.0,13781.4,267.6,22.3]
["Угол равнополочный, ГОСТ 8509-93"]
["25х25х4","Ст.3пс/сп",9.0,48000.0,{"$f":"(D138+D138*3%)/(1000/F138)","v":667.44},{"$f":"ROUNDUP(G138*C138,1)","v":13.5},1.5]
["32х32х4","Ст.3пс/сп",9.0,48000.0,825.648,16.7,1.85]
["40х40х4","Ст.3пс/сп",9.0,48000.0,1156.896,23.4,2.6]
["45х45х4","Ст.3пс/сп",11.7,49000.0,1832.061,36.3,3.1]
["50х50х5","Ст.3пс/сп",11.7,49000.0,2361.996,46.8,4.0]
["63х63х5","Ст.3пс/сп",11.7,48000.0,2951.568,59.7,5.1]
["75х75х6","Ст.3пс/сп",11.7,48500.0,4151.2605,83.1,7.1]
["80х80х6","Ст.3пс/сп",11.7,48500.0,4445.995,89,7.6]
["90х90х7","Ст.3пс/сп",11.7,49000.0,5904.99,117,10.0]
["100х100х7","Ст.3пс/сп",11.7,49000.0,6732.698,133.4,11.4]
["110х110х7","Ст.3пс/сп",11.7,49000.0,7267.68,144,12.3]
["125х125х8","Ст.3пс/сп",11.7,49000.0,9331.903,184.9,15.8]
["140х140х10","Ст.3пс/сп",12.0,49000.0,13142.388,260.4,21.7]
["Швеллер, ГОСТ 8240-97 (ст.09Г2С + 3000 руб/тн)"]
["№ 8","Ст.3пс/сп",11.7,47000.0,{"$f":"(D152+D152*3%)/(1000/F152)","v":4110.009},{"$f":"ROUNDUP(G152*C152,1)","v":84.9},7.25]
["№ 10","Ст.3пс/сп",11.7,47000.0,5044.322,104.2,8.9]
["№ 12","Ст.3пс/сп",11.7,48000.0,6189.888,125.2,10.7]
["№ 14","Ст.3пс/сп",11.7,48000.0,7465.44,151,12.9]
["№ 16","Ст.3пс/сп",11.7,48000.0,8736.048,176.7,15.1]
["№ 18","Ст.3пс/сп",12.0,49000.0,9811.368,194.4,16.2]
["№ 20","Ст.3пс/сп",12.0,61000.0,14174.448,225.6,18.8]
["№ 22","Ст.3пс/сп",12.0,61000.0,16360.932,260.4,21.7]
["№ 24","Ст.3пс/сп",12.0,61000.0,18698.208,297.6,24.8]
["№ 27","Ст.3пс/сп",12.0,61000.0,21261.672,338.4,28.2]
["№ 30","Ст.3пс/сп",12.0,61000.0,24352.908,387.6,32.3]
["Полоса г/к, ГОСТ 103-2003"]
["40х4","Ст.3пс/сп",6.0,50000.0,{"$f":"(D164+D164*3%)/(1000/F164)","v":458.35},{"$f":"ROUNDUP(G164*C164,1)","v":8.9},1.48]
["50х5","Ст.3пс/сп",6.0,53000.0,687.834,12.6,2.1]
["Сетка кладочная, ГОСТ 23279-85"]
["50х50х4","Ст.3пс/сп","0,38х1,5",38500.0,{"$f":"(D167+D167*20%)/(1000/F167)","v":104.412},{"$f":"ROUNDUP(G167*(0.38*1.5),2)","v":2.26},3.95]
["50х50х4","Ст.3пс/сп","0,38х2,0",38500.0,139.986,{"$f":"ROUNDUP(G168*(0.38*2),2)","v":3.03},3.98]
["50х50х4","Ст.3пс/сп","0,51х1,5",38500.0,145.068,{"$f":"ROUNDUP(G169*(0.51*1.5),2)","v":3.14},4.1]
["50х50х4","Ст.3пс/сп","0,51х2,0",38500.0,195.888,{"$f":"ROUNDUP(G170*(0.51*2),2)","v":4.24},4.15]
["50х50х4","Ст.3пс/сп","0,64х1,5",38500.0,186.648,{"$f":"ROUNDUP(G171*(0.64*1.5),2)","v":4.04},4.2]
["50х50х5","Ст.3пс/сп","0,64х1,5",38500.0,284.13,6.15,6.4]
["100х100х4","Ст.3пс/сп","1,0х2,0",38500.0,189.42,{"$f":"ROUNDUP(G173*(1*2),2)","v":4.1},2.05]
["100х100х4","Ст.3пс/сп","1,0х3,0",38500.0,284.13,{"$f":"ROUNDUP(G174*(1*3),2)","v":6.15},2.05]
["100х100х4","Ст.3пс/сп","2,0х3,0",38500.0,{"$f":"(D175+D175*3%)/(1000/F175)","v":487.7565},{"$f":"ROUNDUP(G175*(2*3),2)","v":12.3},2.05]
["100х100х5","Ст.3пс/сп","2,0х3,0",38500.0,{"$f":"(D176+D176*2%)/(1000/F176)","v":742.203},18.9,3.15]
["150х150х4","Ст.3пс/сп","2,0х3,0",38500.0,{"$f":"(D177+D177*3%)/(1000/F177)","v":344.9985},8.7,1.45]
["150х150х5","Ст.3пс/сп","2,0х3,0",38500.0,{"$f":"(D178+D178*2%)/(1000/F178)","v":506.583},12.9,2.15]
["200х200х4","Ст.3пс/сп","2,0х3,0",38500.0,{"$f":"(D179+D179*20%)/(1000/F179)","v":291.06},6.3,1.05]
["200х200х5","Ст.3пс/сп","2,0х3,0",38500.0,{"$f":"(D180+D180*10%)/(1000/F180)","v":393.855},9.3,1.55]
[]
["Цены указаны в рублях с учетом НДС 18%."]
["При покупке до 1 тонны действует наценка 3-5%."]
["К крупным заказам - индивидуальный подход."]
["Осуществляем доставку в регионы."]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}